29 February 2024
SUBJECT: RFQ FOR SUPPLY OF 04 (FOUR) UNIT OF WATER PURIFIER FOR IDCOL
SCHEDULE OF ITEMS AND PRICED QUOTATION FOR WATER PURIFIER
	S.L
	Particular
	Specification
	Quantity (in Pcs)
	Unit Price 

(BDT)
	Total Amount

(BDT)
	Delivery Information

	1.
	Water Purifier
	As Attached Specification
	04
	
	
	Destination
IDCOL Head Office, Level-16,

8, Panthapath, Kawran Bazar, Dhaka-1215

	Total Price (Including VAT @ 7.5%)
	
	

	Taka in words: 


Note: The awarded vendor must complete the delivery within 03 days after issuing purchase order.
___________________________

Company Seal & Signature

Date:

Note: Quotation must be valid for 15 days from the date of submission deadline. 
Documentation Required with the Submission of the Quotation:
The Supplier shall attach with its quotation: 
(a) Copy of updated trade license, 
(b) Copy of e-TIN certificate, 
(c) VAT Reg. Certificate
QUOTATION IN A SEALED ENVELOPE OR THROUGH ELECTRONIC MAIL SHALL BE SUBMITTED TO THE OFFICE OF THE UNDERSIGNED ON OR BEFORE 05 MARCH 2024 AT 02:00 PM.
Sudipto Khatib
Manager, Procurement
Email: khatib@idcol.org
Tel: 9102171-8 (Ext: 6400),  
www.idcol.org
Infrastructure Development Company Limited (IDCOL), 
UTC Building, 16th Floor, 8 Panthapath, Kawran Bazar, Dhaka-1215, Bangladesh

Specification

	Specifications for Water Purifier

	Category
	Specification

	Origin
	To be offer by Vendor

	Manufacture
	Offer by Vendor

	Purified Water Flow Rate (Average)*
	Approximately 15 - 25 Litre per hour

	Membrane Type
	Thin film composite spiral wound

	Pump Type
	Diaphragm pump 24V DC

	% Recovery **
	Typically 25%

	TDS Reduction***
	90% (Min)

	Power Rating
	60 Watts

	Pressure Rating
	10–30 PSI

	Operating Voltage
	100–240 Va.c 50/60 Hz or Manufacturer Standard

	Temperature Range
	10°C- 40°C

	Length of Power Adapter
	1.5 metres

	Total Dissolved Solids in Input Water
	Up to 2000 mg/lit

	Total Hardness
	500 mg/lit (max)

	Iron in Input Water
	0.3 mg/lit (max)

	Turbidity of Input Water
	1 NTU (Max)

	Purification Capacity
	7 to 8 Stages

	Input Water PH Range
	6.5 to 8.5

	Material of Construction
	Food safe, non-toxic, engineering-grade plastics

	Germkill Performance Standard
	Meets stringent international criteria for microbiologically safe drinking water, such as Environmental Protection Agency (EPA), USA

	Product Quantity
	04 (Four) Pcs

	Warranty
	Minimum 03 (Three) Years with manufacture standard warranty.


