
Quotation Submission Letter (Form-1)
[Use Letter-head Pad]

RFQ No: …………………..






Date: dd/mm/yy

To:

Sudipto Khatib
Manager, Procurement 

UTC Building (Level – 16), 8 Panthapath, 
Kawranbazar, Dhaka – 1215 
Phone No: +880-2-222248786-91 (Ext-6400), 
E-mail: khatib@idcol.org 

I/We, the undersigned, offer to supply in conformity with the Terms and Conditions for delivery of the Goods and related services named “……………………………………………”
The total Price of my/our Quotation is BDT [insert amount both in figure and words].
My/Our Quotation shall remain valid for the period stated in the RFQ Document and it shall remain binding upon us and, may be accepted at any time prior to the expiration of its validity period.
I/We declare that I/we have the legal capacity to enter into a contract with you and have not been declared ineligible by the Government of Bangladesh on charges of engaging in corrupt, fraudulent, collusive or coercive practices. Furthermore, I/we am/are aware of Para 21(b) of the Terms and Conditions and pledge not to indulge in such practices in competing for or completion of delivery of Goods.
I/We am/are not submitting more than one Quotation in this RFQ process in my/our own name or other name or in different names. I/We understand that the Purchase Order issued by you shall constitute the Contract and will be binding upon me/us.

I/We have examined and have no reservations to the RFQ Document issued by you on ………………….
I/We understand that you reserve the right to reject all the Quotations or annul the procurement proceedings without incurring any liability to me/us.
	

	Signature of Quotationer with Seal

	Date:



Price Schedule for Goods and Related Services (Form-2)
	Sl. no
	Item Description


	No. of Unit
	Unit Rate or Price


	Total Amount
	Destination for Delivery of Goods

	
	
	
	In figure
	In words
	In figure

In words
	

	1
	2
	3
	4
	5
	6
	7

	1
	Thermal Imaging Camera
	03
	
	
	
	IDCOL HO,

UTC Building

(Level 16), 8 Panthapath, Kawranbazar, Dhaka

	Total Amount for Supply of Goods and related services

(inclusive of VAT @ 7.5% and all applicable taxes; see Note 2 below)
	In figure
	
	

	
	In words
	
	

	Goods to be supplied to                     
	UTC Building (Level 16), 8 Panthapath, Kawran Bazar, Dhaka-1215

	Total Amount in

Taka (in words)
	[enter the Total Amount as in Col.7 above for the delivery of Goods and related services].

	Delivery Offered
	[insert weeks/days] from date of issuing the Purchase Order] 

	Warranty Provided
	[insert weeks/months from date of completion of the delivery; state none if not applicable]


 RFQ No: …………………..
 




Date: dd/mm/yy
[insert number] number corrections made by me/us have been duly initialed in this Price Schedule.  My/Our Offer is valid until dd/mm/yy.
	Signature of Quotationer with Seal
	                    Date: dd/mm/yy

	Name of Quotationer
	


Note:

1. Col. 1, 2, 3, 4 and 8 to be filled in by the Procuring Entity and Col. 5, 6 & 7 by the Quotationer.

2. Rates or Prices shall include profit and overhead and, all kinds of taxes, duties, fees, levies, and other charges earlier paid or to be paid under the Applicable Law, if the Contract is awarded; including transportation, insurance etc. whatsoever up to the point of delivery of Goods and related services in all respects to the satisfaction of the Procuring Entity.         
Technical Specification Compliance Sheet (Form-3)
	Item 1: Thermal Imaging Camera

	SI.

No.
	Criteria
	Requirements
	 Quotationer’s Response

	1
	Brand 
	To be mentioned by the Quotationer
	

	2
	Model
	To be mentioned by the Quotationer (Fluke Ti401 Pro or equivalent)
	

	3
	Country of origin
	To be mentioned by the Quotationer
	

	4
	Infrared resolution
	640 x 480 (307,200 pixels)
	

	5
	IFOV with standard lens (spatial resolution)
	0.93 mRad, D:S 1065:1
	

	6
	Field of view
	34 °H x 24 °V
	

	7
	Minimum focus distance
	15 cm (approx. 6 in)
	

	8
	LaserSharp Auto Focus
	Yes, for consistently in-focus images. Every. Single. Time
	

	9
	Laser distance meter
	Yes, calculates distance to the target for precisely focused images and displays distance on screen
	

	10
	Advanced manual focus
	Yes
	

	11
	Wireless connectivity
	Yes, to PC, iPhone® and iPad® (iOS 4s and later), Android™ 4.3 and up, and WiFi to LAN (where available)
	

	12
	IR-Fusion technology
	Yes, adds the context of the visible details to your infrared image
	

	13
	Ruggedized touchscreen display
	3.5 inch (landscape), 640 x 480 LCD
	

	14
	Ergonomic design
	Pistol-grip design for one-handed use
	

	15
	Thermal sensitivity (NETD)
	<= 0.075 °C at 30 °C target temp (75 mK)
	

	16
	Level and span
	Smooth auto and manual scaling
	

	17
	Touchscreen adjustable level/span
	Yes. Span and level can be easily and quickly set by simply touching the screen
	

	18
	Fast auto toggle between manual and auto modes
	Yes
	

	19
	Fast auto-rescale in manual mode
	Yes
	

	20
	Minimum span (in manual mode)
	2.0 °C (3.6°F)
	

	21
	Minimum span (in auto mode)
	3.0 °C (5.4°F)
	

	22
	Built-in digital camera (visible light)
	5MP
	

	23
	Frame rate
	60 Hz or 9 Hz versions
	

	24
	Laser pointer
	Yes
	

	25
	LED light (torch)
	Yes
	

	26
	Extensive memory options
	Removable 4 GB micro SD memory card, 4 GB internal flash memory, save to USB flash drive capability, upload for permanent storage
	

	27
	Image capture, review, save mechanism
	One-handed image capture, review, and save capability
	

	28
	Image file formats
	bmp, jpeg, is2
	

	29
	Memory review
	Thumbnail and full screen review
	

	30
	Analyze and store radiometric data on a PC
	Yes
	

	31
	Export file formats with Fluke Connect software
	Bitmap (.bmp), GIF, JPEG, PNG, TIFF
	

	32
	Voice annotation
	60 seconds maximum recording time per image; reviewable playback on camera, optional Bluetooth headset available but not required
	

	33
	IR-PhotoNotes
	Yes - 2 images
	

	34
	Text annotations
	Yes. Including standard shortcuts as well as user programmable options
	

	35
	Batteries (field-replaceable, rechargeable)
	Two lithium ion smart battery packs with five-segment LED display to show charge level
	

	36
	Battery life
	2-3 hours per battery (actual life varies depending on settings and usage)
	

	37
	Battery charging time
	2.5 hours to full charge
	

	38
	Battery charging system
	Two-bay battery charger or in-imager charging. Optional 12 V automotive charging adapter
	

	39
	AC operation
	AC operation with included power supply (100 V AC to 240 V AC, 50/60 Hz)
	

	40
	Power saving
	User selectable sleep and power off modes
	

	41
	Temperature measurement range (not calibrated below -10 °C)


	-20 °C to +650 °C (-4 °F to +1,202 °F)
	

	42
	Accuracy
	± 2 °C or 2 % (at 25 °C nominal, whichever is greater)
	

	43
	On-screen emissivity correction
	Yes (both value and table)
	

	44
	On-screen reflected background temperature compensation


	Yes
	

	45
	On-screen transmission correction
	Yes
	

	46
	Standard palettes
	9: Rainbow, Ironbow, Blue-Red, High Contrast, Amber, Amber 

Inverted, Hot Metal, Grayscale, Grayscale Inverted
	

	47
	Ultra Contrast palettes
	9: Rainbow, Ironbow, Blue-Red, High Contrast, Amber, Amber 

Inverted, Hot Metal, Grayscale, Grayscale Inverted
	

	48
	Macro–25 micron lens: 25 MAC2
	Yes
	

	49
	2 x telephoto lens: TELE 2
	Yes
	

	50
	4 x telephoto lens: TELE4
	Yes
	

	51
	Wide angle lens: WIDE 2
	Yes
	

	52
	Color alarms (temperature alarms)
	High temperature, low temperature, and isotherms (within range)
	

	53
	Infrared spectral band
	7.5 µm to 14 µm (long wave)
	

	54
	Operating Temperature
	-10 °C to +50 °C (14 °F to 122 °F)
	

	55
	Storage Temperature
	-20 °C to +50 °C (-4 °F to 122 °F) without batteries
	

	56
	Relative humidity
	10 % to 95 % non-condensing
	

	57
	Center-point temperature measurement
	Yes
	

	58
	Spot temperature
	Hot and cold spot markers
	

	59
	User defined measurement boxes
	1 expandable-contractible measurement box with MIN-MAX-AVG temp display
	

	60
	Hard Case
	Rugged, hard carrying case; soft transport bag
	

	61
	Safety
	IEC 61010-1: Overvoltage category II, Pollution Degree 2
	

	62
	Electromagnetic compatibility
	IEC 61326-1: Basic EM environment. CISPR 11: Group 1, Class A
	

	63
	Vibration
	0.03 g2/Hz (3.8 g), 2.5 g IEC 60068-2-6
	

	64
	Shock
	25 g, IEC 68-2-29
	

	65
	Drop
	Engineered to withstand 2 meter (6.5 feet) drop with standard lens


	

	66
	Size (H x W x L)
	27.7 cm x 12.2 cm x 16.7 cm (10.9 in x 4.8 in x 6.5 in)
	

	67
	Weight (battery included)
	1.04 kg (2.3 lb)
	

	68
	Warranty
	02 years
	


I/We declare to supply Goods and related services offered by me/us fully in compliance with the Technical Specifications and Standards mentioned hereinabove. Catalogue/Brochure of the offered item(s) are also attached. 
	Signature of Quotationer with Seal
	                     Date:  dd/mm/yy


	Name of Quotationer
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