Quotation Submission Letter (Form-1)
[Use Letter-head Pad]

RFQ No: ………………….






Date: dd/mm/yy

To:

Sudipto Khatib
Manager, Procurement 

UTC Building (Level – 16), 8 Panthapath, 
Kawranbazar, Dhaka – 1215 
Phone No: +880-2-222248786-91 (Ext-6400), 

E-mail: khatib@idcol.org 

I/We, the undersigned, offer to supply in conformity with the Terms and Conditions for delivery of the Goods and related services named “……………………………………………”
The total Price of my/our Quotation is BDT [insert amount both in figure and words].
My/Our Quotation shall remain valid for the period stated in the RFQ Document and it shall remain binding upon us and, may be accepted at any time prior to the expiration of its validity period.
I/We declare that I/we have the legal capacity to enter into a contract with you and have not been declared ineligible by the Government of Bangladesh on charges of engaging in corrupt, fraudulent, collusive or coercive practices. Furthermore, I/we am/are aware of Para 21(b) of the Terms and Conditions and pledge not to indulge in such practices in competing for or completion of delivery of Goods.

I/We am/are not submitting more than one Quotation in this RFQ process in my/our own name or other name or in different names. I/We understand that the Purchase Order issued by you shall constitute the Contract and will be binding upon me/us.

I/We have examined and have no reservations to the RFQ Document issued by you on ………………….
I/We understand that you reserve the right to reject all the Quotations or annul the procurement proceedings without incurring any liability to me/us.
	

	Signature of Quotationer with Seal

	Date:




Price Schedule for Goods and Related Services (Form-2)
	Sl. no
	Item Description


	No. of Unit
	Unit Rate or Price


	Total Amount
	Destination for Delivery of Goods

	
	
	
	In figure
	In words
	In figure

In words
	

	1
	2
	3
	4
	5
	6
	7

	1
	PV Analyzer
	02
	
	
	
	IDCOL HO,

UTC Building

(Level 16), 8 Panthapath, Kawranbazar, Dhaka

	Total Amount for Supply of Goods and related services

(inclusive of VAT @ 7.5% and all applicable taxes; see Note 2 below)
	In figure
	
	

	
	In words
	
	

	Goods to be supplied to                     
	UTC Building (Level 16), 8 Panthapath, Kawran Bazar, Dhaka-1215

	Total Amount in

Taka (in words)
	[enter the Total Amount as in Col.7 above for the delivery of Goods and related services].

	Delivery Offered
	[insert weeks/days] from date of issuing the Purchase Order] 

	Warranty Provided
	[insert weeks/months from date of completion of the delivery; state none if not applicable]


 RFQ No: ………………….
 




Date: dd/mm/yy
[insert number] number corrections made by me/us have been duly initialed in this Price Schedule.  My/Our Offer is valid until dd/mm/yy.
	Signature of Quotationer with Seal
	                    Date: dd/mm/yy

	Name of Quotationer
	


Note:

1. Col. 1, 2, 3, 4 and 8 to be filled in by the Procuring Entity and Col. 5, 6 & 7 by the Quotationer.

2. Rates or Prices shall include profit and overhead and, all kinds of taxes, duties, fees, levies, and other charges earlier paid or to be paid under the Applicable Law, if the Contract is awarded; including transportation, insurance etc. whatsoever up to the point of delivery of Goods and related services in all respects to the satisfaction of the Procuring Entity.         
TECHNICAL SPECIFICATION COMPLIANCE SHEET (FORM-3)
	Item 01: PV Analyzer

	SI. No.
	Criteria
	Requirements
	Quotationer’s Response

	1
	Brand 
	To be mentioned by the Quotationer
	

	2
	Model
	To be mentioned by the Quotationer 
(Solmetric PVA 1500HE or equivalent)
	

	3
	Country of origin
	To be mentioned by the Quotationer
	

	4
	Voltage range
	20 to 1500V DC
	

	5
	Voltage Accuracy
	±0.5% ± 0.25V
	

	6
	Current Accuracy
	±0.5% ± 0.04A
	

	 7
	Power Accuracy
	± 1.7% ±1.0W (current z 3A, module efficiency <19%)
	

	8
	I-V trace Points
	100 or 500 Selectable
	

	9
	I-V sweep Duration
	0.05 to 2s. Typically 0.2s for PV Strings.
	

	10
	Operating Temperature (ambient)
	32 to 113° F (0 to +45° C
	

	11
	Weight
	16 lb
	

	12
	Dimensions
	21’x 8.5" x 6"
	

	13
	Safety and Regulatory
	CAT III 1500V
	

	Maximum Current (lsc)

	14
	Model Efficiency <19
	30 A DC
	

	15
	Model Efficiency ≥ 19%
	30 A DC
	

	Measurement Throughput

	16
	Sweep-to-sweep delay (@Voc ≤ 1350V)
	<9S
	

	17
	Max # 1-V sweeps per hour (@ Voc ≤ 1350V)
	400 Sweeps/hr
	

	18
	Max megawatts measured per hour 

(assume reference PV system with Voc = 1300V, Vmp = 11 OOV, Imp = 25A, 16 strings per combiner, 5 min to move next combiner with no measurements. No direct sunlight on 1-V unit)
	3.5M W/hr
	

	Thermal Capacity--# 1-V Sweeps Before PVA Must Cool Down 

	19
	77° Ambient, 18s Sweep-to-sweep delay
	Unlimited
	

	20
	77° Ambient, 9s Sweep-to-sweep delay
	Unlimited
	

	21
	113° Ambient, 18s Sweep-to-sweep delay
	450
	

	22
	113° Ambient, 9s Sweep-to-sweep delay
	330
	

	SolSensor

	23
	Irradiance Accuracy
	±2% Typical (600 to 1500 W/m2, Si cells)
	

	24
	Cell Temperature Accuracy
	± 2° C typical, Smart Temp Method
	

	25
	Tilt Accuracy
	± 2° Typical (0 to 45°)
	

	26
	Update Interval
	Irradiance: 0.1 s, Temperature: 1 s
	

	27
	Wireless Range
	100m (Open line of sight)
	


I/We declare to supply Goods and related services offered by me/us fully in compliance with the Technical Specifications and Standards mentioned hereinabove. Catalogue/Brochure of the offered item(s) are also attached. 
	Signature of Quotationer with Seal
	                     Date:  dd/mm/yy



	Name of Quotationer
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